{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["MERC_0907_DRV","MERC_0907_UI_无WIFI"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MERC_0907_DRV","index":0,"n_rows":76,"n_cols":15,"rows_kept":76,"cut":false,"hidden":false,"merged":[[75,2,75,11],[0,0,2,2],[0,12,0,14],[1,5,1,7],[1,12,1,13],[2,5,2,7],[2,11,2,14],[1,3,1,4],[2,3,2,4],[0,3,0,11],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,3,4],[3,5,3,6],[3,7,4,7],[3,13,4,13],[3,14,4,14],[3,8,4,8],[3,9,4,9],[3,10,4,10],[3,11,4,11],[3,12,4,12]]}
[null,null,null,"PCBA BOM表"]
[null,null,null,"项目编号：",null,"MERC_0907_DRV",null,null,"版本号：","V1.01","BOM编制人：",null,"编制时间：",null,"2026.03.26"]
[null,null,null,"客户名称：",null,"健仕",null,null,"客板信息：","制冰机-驱动板-欧标","项目描述："]
["序号","物料需求","规格","建议物料",null,"备选物料",null,"类别","封装","位号","NC","备注","数量","单价","合计"]
[null,null,null,"料号或描述","品牌","料号或描述","品牌"]
[1,"51R 1%",0.01,"不限","不限","/","/","贴片电阻","R0603","R2, R5, R11, R13, R15, R17",null,null,6]
[2,"68R 1%",0.01,"不限","不限","/","/","贴片电阻","R0603","R18, R19",null,null,2]
[3,"100R 5%",0.05,"不限","不限","/","/","贴片电阻","R0603","R6, R7",null,null,2]
[4,"1K 5%",0.05,"不限","不限","/","/","贴片电阻","R0603","R21, R48",null,null,2]
[5,"7K5 1%",0.01,"不限","不限","/","/","贴片电阻","R0603","R23",null,null,1]
[6,"10K 5%",0.05,"不限","不限","/","/","贴片电阻","R0603","R4, R9",null,null,2]
[7,"10K 1%",0.01,"不限","不限","/","/","贴片电阻","R0603","R22",null,null,1]
[8,"24K 1%",0.01,"不限","不限","/","/","贴片电阻","R0603","R20",null,null,1]
[9,"100K 1%",0.01,"不限","不限","/","/","贴片电阻","R0603","R1, R3, R10, R12, R14, R16, R8",null,null,7]
[10,"10R 5%",0.05,"不限","不限","/","/","贴片电阻","R0805","R40, R43",null,null,2]
[11,"15K 1%",0.01,"不限","不限","/","/","贴片电阻","R0805","R46",null,null,1]
[12,"27K 1%",0.01,"不限","不限","/","/","贴片电阻","R0805","R45",null,null,1]
[13,"75K 1%",0.01,"不限","不限","/","/","贴片电阻","R0805","R44",null,null,1]
[14,"NC/0R ",0.01,"不限","不限","/","/","贴片电阻","R1206",null,"R26","110V倍压跳线选择",0]
[15,"33R 5%",0.05,"不限","不限","/","/","贴片电阻","R1206","R29, R30",null,null,2]
[16,"62R 5%",0.05,"不限","不限","/","/","贴片电阻","R1206","R36, R37, R38, R39",null,null,4]
[17,"20K 5%",0.05,"不限","不限","/","/","贴片电阻","R1206","R34, R35",null,null,2]
[18,"330K 5%",0.05,"不限","不限","/","/","贴片电阻","R1206","R24, R28, R31, R32, R33",null,null,5]
[19,"680K 1%",0.01,"不限","不限","/","/","贴片电阻","R1206","R25, R27",null,null,2]
[20,"100mR 1%",0.01,"不限","不限","/","/","贴片电阻","R1210","R47",null,null,1]
[21,"360mR 1%",0.01,"不限","不限","/","/","贴片电阻","R2010","R49, R50",null,null,2]
[22,"0.02R 1%",0.01,"不限","不限","/","/","贴片电阻","R2512","RS1",null,null,1]
[23,"101/50V","X7R,10%;50V","不限","不限","/","/","贴片电容","C 0603","C3",null,null,1]
[24,"102/50V","X7R,10%;50V","不限","不限","/","/","贴片电容","C 0603","C16, C17, C18, C19, C20, C21, C13",null,null,7]
[25,"103/50V","X7R,10%;50V","不限","不限","/","/","贴片电容","C 0603","C4, C5",null,null,2]
[26,"104/50V","X7R,10%;50V","不限","不限","/","/","贴片电容","C 0603","C10, C12",null,null,2]
[27,"1uF/25V","X7R,10%;25V","不限","不限","/","/","贴片电容","C 0603","C1",null,null,1]
[28,"4.7uF/25V","X5R,10%;25V","不限","不限","/","/","贴片电容","C 0603","C2",null,null,1]
[29,"10uF/16V","X5R,10%;16V","不限","不限","/","/","贴片电容","C 0603","C11",null,null,1]
[30,"20pF/50V","C0G,5%;50V","不限","不限","/","/","贴片电容","C 0805","C8",null,null,1]
[31,"10uF/50V","X5R,10%;50V","不限","不限","/","/","贴片电容","C 0805","C9, CL1",null,null,2]
[32,"47pF/1KV","C0G,5%;1KV","不限","不限","/","/","贴片电容","C 1206","C14",null,null,1]
[33,"470pF/1KV","X7R,10%;1KV","不限","不限","/","/","贴片电容","C 1206","C6",null,null,1]
[34,"10nF/1kV","X7R,10%;1KV","不限","不限","/","/","贴片电容","C 1206","C7",null,null,1]
[35,"NC/100nF/450V","X7R,10%;450V","不限","不限","/","/","贴片电容","C 1206",null,"C15, C22","不焊接",0]
[36,"KBP310",null,"不限","不限","/","/","整流桥堆","DB/GBP310/3.8","D1",null,null,1]
[37,"MBRF20200CT",null,"不限","不限","/","/","肖特基二极管","TO-220F","D2, D4",null,null,2]
[38,"S3MB",null,"不限","不限","/","/","贴片二极管","SMB","D6",null,null,1]
[39,"1N4007W（A7）",null,"不限","不限","/","/","贴片二极管","SOD123","D7",null,null,1]
[40,"S2M",null,"不限","不限","/","/","贴片二极管","SMA","D8",null,null,1]
[41,"T 3.15A 250VAC",null,"不限","不限","/","/","保险丝","FUSE-TH_L8.4-W4.3-P5.08-D1.0","F1",null,null,1]
[42,"78L05","150mA","不限","不限","/","/","LDO电源管理芯片 150mA","SOT89_M","U4",null,null,1]
[43,"PH2.0_5P",null,"不限","不限","/","/","接插件","CON_PH2.0mm_5P","J1",null,null,1]
[44,"XH2.54-LI-2P",null,"不限","不限","/","/","接插件","XH2.54-LI-2P","J3, J4",null,null,2]
[45,"XH2.54-LI-3P",null,"不限","不限","/","/","接插件","XH2.54-LI-3P","J5",null,null,1]
[46,"XH2.54-LI-5P",null,"不限","不限","/","/","接插件","XH2.54-LI-5P","P1",null,null,1]
[47,"VH3.96-2P",null,"不限","不限","/","/","接插件","VH3.96-2P","J2",null,null,1]
[48,"VH3.96-3P",null,"不限","不限","/","/","接插件","VH3.96-3P","M1",null,null,1]
[49,"G630_09_3T",null,"不限","不限","/","/","插片6.3mm","6.3MM P_5mm","J7, J8, J9, J10",null,null,4]
[50,"温度传感器（焊接）",null,"不限","不限","/","/","温度传感器外置引线",null,"J6",null,null,1]
[51,"1.5uH共模电感 绕线线径0.5mm","300mV/1KHZ ≥1.5uH \nT10*6*5","不限","不限","/","/","镍锌磁环共模电感","T10X6X5 P3.5X7mm","T4",null,"比样品线径要粗，切记",1]
[52,"80uH ±30%共模电感 绕线线径0.7mm","300mV/1KHZ 80uH \nT10*6*5","不限","不限","/","/","镍锌磁环共模电感","T10X6X5 P3.5X7mm","T1",null,"按样品做",1]
[53,"SQ1515 45mH共模电感","300mV/1KHZ ≥45mH  SQ1515","不限","不限","/","/","共模电感","SQ1515 P8x10mm","T3",null,"按样品做",1]
[54,"PQ2625 CE变压器",null,"不限","不限","/","/","安规变压器PQ2625 6+4","PQ2625 CE","T2",null,null,1]
[55,"2.5D-11","温敏电阻银基","206RV366","科尼盛","/","/","NTC温敏电阻","2.5D-11","NTC1",null,null,1,"昇擎"]
[56,"10uF/50V",">=3000H 105℃","DGA050M106C113T1AA","科尼盛","/","/","电解电容","CAP 2.5*5*11mm","CE3",null,null,1,"昇擎"]
[57,"150uF/200V",">=3000H 105℃","DHG200M157L2C0S1AA","科尼盛","/","/","电解电容","CAP 5.0*13*22mm","CD1, CD2",null,null,2,"昇擎"]
[58,"1000uF/25V",">=3000H 105℃","DHG025M108H200C4AA","科尼盛","/","/","电解电容","CAP 5.0*10*20mm","CE1, CE2",null,null,2,"昇擎"]
[59,"470uF/25V",">=3000H 105℃","DHG025M477G120T1AA","科尼盛","/","/","电解电容","CAP 3.5*8*12mm","CE4",null,null,1,"昇擎"]
[60,"474/275VAC",null,"MPX474K31C3KN206B0","科尼盛","/","/","X2电容","CX 13X12X6 P 10mm","CX1",null,null,1,"昇擎"]
[61,"224/275VAC",null,"MPX224K31C3KN206B","科尼盛","/","/","X2电容","CX 13X12X6 P 10mm","CX2",null,null,1,"昇擎"]
[62,"2.2nF/300V",null,"70Y20157","科尼盛","/","/","Y2电容","CY P_7.5MM","CY1, CY2, CY5",null,null,3,"昇擎"]
[63,"4.7nF/300V",null,"70Y20100","科尼盛","/","/","Y2电容","CY P_7.5MM","CY3, CY4",null,null,2,"昇擎"]
[64,"10D471K",null,"68RV0637","科尼盛","/","/","压敏电阻","10D471","RV1",null,null,1,"昇擎"]
[65,"SGP013E8S8PG",null,"SGP013E8S8PG","昇擎","/","/","主控MCU","ssop24","U1",null,null,1,"昇擎"]
[66,"BSS84",null,"BSS84PK","冠禹","/","/","P-MOSFET","SOT23","Q2",null,null,1,"昇擎"]
[67,"KS3256AA",null,"KS3256AA","冠禹","/","/","N-MOSFET","SOT23","Q3",null,null,1,"昇擎"]
[68,"YHT030NP030L5",null,"YHT030NP030L5","炎黄","R30G30","/","N+P合封mosfet","DFN5X6","Q1, Q4, Q5",null,null,3,"昇擎"]
[69,"ULN2003D",null,"ULN2003-SOA-R-R","海速芯","/","/","达林顿阵列","SOP16","U2",null,null,1,"昇擎"]
[70,"LCW620H",null,"LCW620H","领芯微","/","/","ACDC电源管理芯片","ESOP6","U3",null,null,1,"昇擎"]
[71,"PCB","尺寸：122mmX32mm ；材料：FR-4 ；板层：2层；铜厚：1盎司（oz）；板厚：1.6mm;铅喷锡绿油白字-过孔盖油-1oz-过CQC",{"$nulls":9},{"$f":"SUM(M6:M75)","v":116}]

{"sheet":"MERC_0907_UI_无WIFI","index":1,"n_rows":34,"n_cols":15,"rows_kept":34,"cut":false,"hidden":false,"merged":[[33,2,33,11],[0,0,2,2],[0,3,0,11],[0,12,0,14],[1,5,1,7],[1,12,1,13],[2,5,2,7],[2,11,2,14],[1,3,1,4],[2,3,2,4],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,3,4],[3,5,3,6],[3,7,4,7],[3,13,4,13],[3,14,4,14],[3,8,4,8],[3,9,4,9],[3,10,4,10],[3,11,4,11],[3,12,4,12]]}
[null,null,null,"PCBA BOM表"]
[null,null,null,"项目编号：",null,"MERC_0907_UI",null,null,"版本号：","V1.01","BOM编制人：",null,"编制时间：",null,"2026.03.26"]
[null,null,null,"客户名称：",null,"健仕",null,null,"客板信息：","制冰机-UI板","项目描述：","无wifi模块和UV灯"]
["序号","物料需求","规格","建议物料",null,"备选物料",null,"类别","封装","位号","NC","备注","数量","单价","合计"]
[null,null,null,"料号或描述","品牌","料号或描述","品牌"]
[1,"1K 5%",0.05,"不限","不限","/","/","贴片电阻","R0603","R1, R2, R6, , R10, R11, R12, R15, ","R8, R9, R16, R19",null,7]
[{"$f":"A6+1","v":2},"4.7K 1%",0.01,"不限","不限","/","/","贴片电阻","R0603","R18",null,null,1]
[{"$f":"A7+1","v":3},"6.8K 1%",0.01,"不限","不限","/","/","贴片电阻","R0603","R3, R4, R5, R7",null,null,4]
[4,"10K 5%",0.05,"不限","不限","/","/","贴片电阻","R0603",null,"R17, R20, R21, R24, R25",null,0]
[5,"10K 1%",0.01,"不限","不限","/","/","贴片电阻","R0603",null,"R22",null,0]
[6,"20K 1%",0.01,"不限","不限","/","/","贴片电阻","R0603",null,"R23",null,0]
[7,"24K 1%",0.01,"不限","不限","/","/","贴片电阻","R0603",null,"RP3",null,0]
[8,"75K 1%",0.01,"不限","不限","/","/","贴片电阻","R0603",null,"RP2",null,0]
[9,"100K 5%",0.05,"不限","不限","/","/","贴片电阻","R0603",null,"RP1",null,0]
[10,"1.3M 1%",0.01,"不限","不限","/","/","贴片电阻","R0603","R14",null,null,1]
[11,"330R 5%",0.05,"不限","不限","/","/","贴片电阻","R0805","R13",null,null,1]
[12,"47pF/50V","C0G,5%","不限","不限","/","/","贴片电容","C0603",null,"CP2",null,0]
[13,"102/50V","X7R,10%","不限","不限","/","/","贴片电容","C0603","C4",null,null,1]
[14,"104/50V","X7R,10%","不限","不限","/","/","贴片电容","C0603","C1, C3, C7","C6, CP1",null,3]
[15,"10uF/25V","X5R,10%","不限","不限","/","/","贴片电容","C0603","C2","C5, C8",null,1]
[16,"47uF/25V","X5R,20%","不限","不限","/","/","贴片电容","C1206",null,"CP3, CP4",null,0]
[17,"10uH ","2.2A,20%","不限","不限","/","/","功率电感","SMD,4.2x4.4mm",null,"LP1",null,0]
[18,"LED_W",null,"不限","不限","/","/","白色发光二极管","LED 0603W","LED1, LED2, LED3, LED4, LED5, LED6","'LED7",null,6]
[19,"MMBT5551",null,"不限","不限","/","/","NPN 三极管","SOT23",null,"Q1, Q2",null,0]
[20,"2N7002K",null,"不限","不限","/","/","N-MOSFET","SOT23",null,"Q3, Q4",null,0]
[21,"WBR3",null,"WBR3","涂鸦","/","/","TUYA模块","TUYA_WBR3",null,"U2",null,0]
[22,"触摸按键方形","宽15长16.5高15宽上出脚，线径0.7","不限","不限","/","/","触摸按键","TB_15-双针-方","TK1, TK2, TK3, TK4",null,null,4]
[23,"ZH1.5_2PWT  ",null,"不限","不限","/","/","贴片接插件","CONN-SMD_2P-P1.50_ZX-ZH1.5-3PWT",null,"J2",null,0]
[24,"ZH1.5_3PWT",null,"不限","不限","/","/","贴片接插件","CONN-SMD_3P-P1.50_ZX-ZH1.5-3PWT","J1, J3",null,null,2]
[25,"ZH1.5_5PWT",null,"不限","不限","/","/","贴片接插件","CONN-SMD_5P-P1.50_ZX-ZH1.5-3PWT","P1",null,null,1]
[26,"Header 4",null,"不限","不限","/","/","调试口","HDR1X4",null,"P2","调试口不焊接",0]
[27,"SGT8M004G4S7",null,"SGT8M004G4S7","昇擎","/","/","主控MCU","SSOP28","U1",null,null,1,"昇擎"]
[28,"LCW518X",null,"LCW518X","领芯微","/","/","DCDC电源管理","SOT23-6",null,"UP1",null,0,"昇擎"]
[29,"PCB","尺寸：122mmX32mm ；材料：FR-4 ；板层：2层；铜厚：1盎司（oz）；板厚：1.6mm "]