{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["MERC0102-DRV"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MERC0102-DRV","index":0,"n_rows":39,"n_cols":10,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,8],[38,2,38,6]]}
["MERC0102-DRV V1.05"]
["序号","规格","主选","备选","注释","封装","位号","DNP","备注说明","数量"]
[1,"0R/NC",null,null,"电阻","R0603",null,"R1","不焊接",0]
[2,"51R",null,null,"电阻","R0603","R5, R6, R7, R13, R14, R15",null,null,6]
[3,"68R",null,null,"电阻","R0603","R19, R20",null,null,2]
[4,"1K",null,null,"电阻","R0603","R24, R25, R31, R39, R40, R47, R48, R49",null,null,8]
[5,"2.4K/NC",null,null,"电阻","R0603",null,"R28, R33, R36","不焊接",0]
[6,"4K7",null,null,"电阻","R0603","R42",null,null,1]
[7,"10K",null,null,"电阻","R0603","R30, R37, R38, R41, R43, R44, R45, R46","R23","不焊接",8]
[8,"15K 1%",null,null,"电阻","R0603","R34",null,null,1]
[9,"20K/NC",null,null,"电阻","R0603",null,"R27, R32, R35","不焊接",0]
[10,"100K",null,null,"电阻","R0603","R9, R10, R11, R16, R17, R18",null,null,6]
[11,"220K 1%",null,null,"电阻","R0603","R29",null,null,1]
[12,"5.1R 5% 0805",null,null,"电阻","R0805","R26",null,null,1]
[13,"10R",null,null,"电阻","R0805","R3",null,null,1]
[14,"2K",null,null,"电阻","R0805","R2",null,null,1]
[15,"75mR_2512 1%",null,null,"电阻","R2512","R21",null,null,1]
[16,"101/25V",null,null,"电容","C0603","C8, C16, C18, C21",null,null,4]
[17,"102/25V",null,null,"电容","C0603","C11",null,null,1]
[18,"103/25V",null,null,"电容","C0603","C20",null,null,1]
[19,"104/25V",null,null,"电容","C0603","C3, C4, C10, C15, C19, C23, C29",null,null,7]
[20,"2.2uF/25V",null,null,"电容","C0603","C12, C13, C14",null,null,3]
[21,"105/25V",null,null,"电容","C0603","C27",null,null,1]
[22,"10uF/25V",null,null,"电容","C0805","C7, C17, C22",null,null,3]
[23,"22uF/25V",null,null,"电容","C0805","C25, C26, C30",null,null,3]
[24,"4.7uF/100V",null,null,"电容","C1210","C1",null,null,1]
[25,"DSS210",null,null,"肖特基","SOD123","D2",null,null,1]
[26,"SD103AWS",null,null,"二极管/高效率/通用","SOD323","D3, D4, D5",null,null,3]
[27,"1N4007",null,null,"二极管/高效率/通用","SOD123","D6",null,null,1]
[28,"330uH",null,null,"贴片电感","IND-SMD_L4.0-W4.0","L1",null,null,1]
[29,"HC-MX3.0-2*5AW",null,null,"接插件","C3004WR_2X5P","P1",null,null,1]
[30,"KS6410HB",null,null,"Dual N MOSFET","SOP8_M","Q1, Q2, Q3",null,"自备",3]
[31,"MMBT5401",null,null,"PNP General Purpose Amplifier","SOT-23","Q4",null,null,1]
[32,"2N7002",null,null,"N-Channel MOSFET","SOT-23","Q5",null,null,1]
[33,"HTB7316",null,null,"DCDC电源管理芯片","SOP8_M","U1",null,"自备",1]
[34,"78L05",null,null,"LDO稳压芯片","SOT89_M","U2",null,null,1]
[35,"SGP32F011K6T8NE",null,null,"主控MCU","LQFP32 7X7_N","U3",null,"自备",1]
[36,"MA7022BAA",null,null,"霍尔检测芯片","SOT-23","U4, U5, U6",null,"自备",3]
[37,"PCB","尺寸：58mmX42mm ；材料：FR-4 ；板层：2层；铜厚：1盎司（oz）；板厚：1.6mm",{"$nulls":6},{"$f":"0.58*0.42","v":0.24359999999999998}]