{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["MERC0102-PWR"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MERC0102-PWR","index":0,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[0,0,0,8],[60,2,60,6]]}
["MERC0102-PWR V1.03"]
["序号","规格","主选","备选","注释","封装","位号","DNP","备注说明","数量"]
[1,"10R",null,null,"电阻","R0805","R14, R24",null,null,2]
[{"$f":"A3+1","v":2},"27R",null,null,"电阻","R0805","R23",null,null,1]
[{"$f":"A4+1","v":3},"470R",null,null,"电阻","R0805","R25",null,null,1]
[4,"1K 1%",null,null,"电阻","R0805","R15, R18, R21, R22",null,null,4]
[5,"2K 1%",null,null,"电阻","R0805","R28",null,null,1]
[6,"10K",null,null,"电阻","R0805","R33",null,null,1]
[7,"18K 1%",null,null,"电阻","R0805","R26",null,null,1]
[8,"27K 1%",null,null,"电阻","R0805","R19",null,null,1]
[9,"68K  1%",null,null,"电阻","R0805","R16, R20",null,null,2]
[10,"NC",null,null,"电阻","R0805",null,"R27","不焊接",0]
[11,"1R  1%",null,null,"电阻","R1206","R29, R30, R31, R32, R38",null,null,5]
[12,"2R",null,null,"电阻","R1206","R17",null,null,1]
[13,"33R",null,null,"电阻","R1206","R2, R3",null,null,2]
[14,"68R",null,null,"电阻","R1206","R34, R35",null,null,2]
[15,"20K",null,null,"电阻","R1206","R9, R10",null,null,2]
[16,"33K",null,null,"电阻","R1206","R4, R5, R7, R8",null,null,4]
[17,"330K",null,null,"电阻","R1206","R11, R12, R13",null,null,3]
[18,"680K",null,null,"电阻","R1206","R1, R6",null,null,2]
[19,"101/50V/NC",null,null,"电容","C0805",null,"C6","不焊接",0]
[20,"221/250V/NC",null,null,"电容","C0805",null,"C3","不焊接",0]
[21,"221/50V",null,null,"电容","C0805","C8",null,null,1]
[22,"102/50V",null,null,"电容","C0805","C7",null,null,1]
[23,"103/25V",null,null,"电容","C0805","C16, C17",null,null,2]
[24,"104/50V",null,null,"电容","C0805","C5",null,null,1]
[25,"105/50V",null,null,"电容","C0805","C4, C13",null,null,2]
[26,"4.7uF/25V",null,null,"电容","C0805","C12",null,null,1]
[27,"22uF/16V",null,null,"电容","C0805","C14, C15",null,null,2]
[28,"102/1KV",null,null,"电容","C1206","C1",null,null,1]
[29,"10uF/100V/NC",null,null,"电容","C1210",null,"C10","不焊接",0]
[30,"10uF/50V","KNSCHA 10uF/50V",null,"电解电容（插件）","CE5X11 P_2.5mm","CE5",null,"自备",1]
[31,"82uF/400V","KNSCHA 82uF/400V",null,"电解电容（插件）","CE18X25 P_7.5mm","CE1",null,"自备",1]
[32,"470uF/50V","KNSCHA470uF/50V",null,"电解电容（插件）","CE10X20 P_5mm","CE6",null,"自备",1]
[33,"680uF/50V","KNSCHA 680uF/50V",null,"电解电容（插件）","CE12.5X25 P_5.0mm","CE3, CE4",null,"自备",2]
[34,"334/275VAC","KNSCHA 334/275VAC",null,"安规X电容（插件）","CX104/275V/10H","CX1",null,"自备",1]
[35,"102/250V","KNSCHA 102 250V Y电容",null,"安规Y电容（插件）","CY_7.5mm","CY3, CY4",null,"自备",2]
[36,"102/630V","KNSCHA 102 630V CBB",null,"CBB直插电容；脚距P=5mm","C103/400V/5H","C2",null,"自备",1]
[37,"100uH",null,null,"贴片电感","L1210","L3",null,null,1]
[38,"MBRF20200",null,null,"肖特基（插件）","TO-220","D1",null,null,1]
[39,"M7",null,null,"二极管/高效率/通用","SMA","D2",null,null,1]
[40,"1N4007",null,null,"二极管/高效率/通用","SOD123","D3, D4, D6",null,null,3]
[41,"DSS210",null,null,"肖特基","SOD123","D5",null,null,1]
[42,"KBP310","Yjsemi KBP310",null,"直插桥堆（插件）","DB/GBP310/3.8","BD1",null,"自备",1]
[43,"MMBT5551",null,null,"NPN三极管","SOT-23","Q1",null,null,1]
[44,"MMBT5401",null,null,"PNP三极管","SOT-23","Q3",null,null,1]
[45,"YH10N65F","YH10N65F",null,"N-Channel MOSFET（插件）","TO-220","Q2",null,"自备",1]
[46,"T5A250V",null,null,"保险丝（插件）","F4_8.5","F1",null,null,1]
[47,"20mH","20mH",null,"共模电感（插件）","P_1.0x0.8_H_19mm","L1",null,"自备",1]
[48,"6uH","6uH",null,"共模电感（插件）","L-6_15","L2",null,"自备",1]
[49,"14D561",null,null,"压敏电阻（插件）","14D561K","MOV1",null,null,1]
[50,"2.5D11",null,null,"温敏电阻（插件）","2.5D-11","RT1",null,null,1]
[51,"EE30 5+5","EE30 5+5",null,"变压器磁芯EE30 骨架5+5（插件）","T-EE30_5+5","T1",null,"自备",1]
[52,"LTV_1008","UMW LTV1008",null,"光耦","SOP_4_2.54","U1",null,null,1]
[53,"SGT0076BA","SGT0076BA",null,"电源主控IC","SOT23-6","U2",null,"自备",1]
[54,"TL431",null,null,"稳压IC","SOT23","U3",null,null,1]
[55,"ES4903","ES4903",null,"线性霍尔（直插）","TO-92","U4",null,"自备",1]
[56,"HTB7325C",null,null,"DC/DC电源IC","SOP8","U5",null,"自备",1]
[57,"NV-2WA",null,null,"接插件","CONN-TH_2P-P5.00_XD-NV-2AW-G",null,"P1","直接焊线",0]
[58,"VH_3WA",null,null,"接插件","CONN-TH_3P-P3.96_HX-VH3.96-3P-WZ",null,"P2","直接焊线",0]
[59,"PCB","尺寸：85mmX74mm ；材料：FR-4 ；板层：2层；铜厚：1盎司（oz）；板厚：1.6mm",{"$nulls":6},{"$f":"0.85*0.74","v":0.629}]