{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["MERC0203E-DRV-V2.10"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MERC0203E-DRV-V2.10","index":0,"n_rows":48,"n_cols":10,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
["需求","规格","建议物料","备选物料","类别","封装","位号","NC","备注","数量"]
["1nF/25V","1nF",null,null,"贴片电容","C0603","C1, C7, C13, C16, C17, C19, C21, C22",null,null,8]
["1uF/25V","1uF",null,null,"贴片电容","C0603","C2",null,null,1]
["100nF/50V","100nF",null,null,"贴片电容","C0603","C4, C5, C8, C14, C15, C18",null,null,6]
["2.2uF/25V","2.2uF",null,null,"贴片电容","C0603","C9, C10, C11, C20",null,null,4]
["10uF/25V","10uF",null,null,"贴片电容","C0805","C3, C12",null,null,2]
["10nF/500V","10nF",null,null,"贴片电容","C1206","CY1",null,null,1]
["100nF/500V","100nF",null,null,"贴片电容","C1206","C6",null,null,1]
["100nF/500V","100nF",null,null,"贴片电容","C1812","CH1",null,null,1]
["100uF/25V","100uF",null,null,"直插电解电容","CAP 2.0*5*11","EC3",null,null,1]
["47uF/400V","47uF",null,null,"直插电解电容","CAP 5.0*12.5*20","EC1, EC2",null,"高频",2]
["680nF","680nF",null,null,"安规电容","CAp-X2-P_10-12*13*8","CX1",null,null,1]
["10R","10R",null,null,"贴片电阻","R0603",null,"R19, R20, R21","",0]
["1K/1%","1K/",null,null,"贴片电阻","R0603","R2, R38, R44, R46",null,null,4]
["330R","330R",null,null,"贴片电阻","R0603","R10",null,null,1]
["68R/1%","68R",null,null,"贴片电阻","R0603","R11, R12, R22, R29, R33, R34",null,null,6]
["270R/1%","270R",null,null,"贴片电阻","R0603","R13, R14, R15, R23, R24, R25",null,null,6]
["10K/1%","10K",null,null,"贴片电阻","R0603","R1, R16, R17, R18, R26, R27, R28, R36, R39, R45, R47",null,null,11]
["100R","100R",null,null,"贴片电阻","R0603","R35, R43, R48",null,null,3]
["3.65K/1%","3.65K",null,null,"贴片电阻","R0603","R40",null,null,1]
["20K","20K",null,null,"贴片电阻","R0603","R41",null,null,1]
["10R","10R",null,null,"贴片电阻","R0805","R7",null,null,1]
["560K/1%","560K",null,null,"贴片电阻","R1206","R37, R42",null,null,2]
["110R","110R",null,null,"贴片电阻","R1206","R8, R9",null,null,2]
["200K","200K",null,null,"贴片电阻","R1206","R3",null,null,1]
["680K","680K",null,null,"贴片电阻","R1206","R4, R6",null,null,2]
["300mR","300mR",null,null,"电流采样电阻","R0805","R5",null,null,1]
["150mR/1%/250mW","150mR","建议使用200ppm以内低温漂采样电阻，不少于1/4W",null,"电流采样电阻","R1206","R30, R31, R32",null,null,3]
["LED_R","红灯",null,null,"发光二极管","LED 0603","LED1, LED3, LED5",null,null,3]
["LED_W","白灯",null,null,"发光二极管","LED 0603","LED2, LED4, LED6",null,null,3]
["US1MW","US1MW",null,null,"超快恢复二极管","SOD-323",null,"D1, D2, D3",null,0]
["DB207S","DB207S",null,null,"整流桥","DBS","DB1",null,null,1]
["47uH",null,"220V-2.5A(可以更换封装)",null,"功率电感","L1040-SMD-L11.6-W10.1","LS1",null,null,1]
["贴片接线端子","间距1.25，贴片","COOL, NTC",null,"接线端子","CON-SMD_2P-P1.25-HC","P2","P1",null,1]
["1mH/300mA","1mH,±20%,300mA,4.5Ω ",null,null,"功率电感","L6045S","L2",null,null,1]
["3.15A/250V贴片",null,null,null,"一次性保险丝","FUSE-SMD_L6.1-W2.5","FS1",null,null,1]
["3H4_B","过零光耦",null,null,"过零光耦","SOP-4-P1.27","U1",null,null,1]
["YH5N50","N沟道,500V",null,null,"场效应管","TO252","Q1, Q2, Q3, Q4, Q5, Q6",null,"昇擎",6]
["M3052","可控硅控制光耦",null,null,"光耦","SOP4_M","U4",null,null,1]
["HD1520","ACDC",null,null,"ACDC电源","SOP8_M","U2",null,"昇擎",1]
["78L05",null,null,null,"线性稳压器","SOT89_M","U3",null,null,1]
["3313B","3313B",null,null,"电机控制IC","SOP8_M","U5, U7, U8",null,"昇擎",3]
["37S01","主控MCU",null,null,"MCU","SSOP24","U6",null,"昇擎",1]
["轻触开关-5.1x5.1","5.1*5.1*1.7H",null,null,"铜头按钮","SW-SMD_4P-L5.1-W5.1-P3.70-LS6.5-TL-2","S1, S2",null,null,2]
["BT138-800E",null,null,null,"可控硅","TO220A","BT1",null,null,1]
["7D471",null,null,null,"压敏电阻","VR","RV1",null,null,1]
["3D-9",null,null,null,"热敏电阻","NCT_7p5","NTC1",null,null,1]
["PCB双面板","68.1*67.4板厚1.2",null,null,"PCB板",{"$nulls":4},1]