{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["MERC-0241"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MERC-0241","index":0,"n_rows":63,"n_cols":10,"rows_kept":63,"cut":false,"hidden":false,"merged":[[0,0,0,9],[12,0,12,9]]}
["MERC-0241-UI  UI板-板厚1.0mm"]
["需求","规格","建议物料","备选物料","类别","封装","位号","NC","备注","数量"]
["100nF/50V","100nF",null,null,"贴片电容","C0603","C1, C3",null,null,2]
["1nF/25V","1nF",null,null,"贴片电容","C0603","C2",null,null,1]
["1K/1%","1K",null,null,"贴片电阻","R0603","R1, R2, R3, R4, R5, R6, R7, R8",null,null,8]
["4Pin贴片排座","2x2P-P2.00",null,null,"贴片端子","CON-SMD_2x2P-P2.00-PZ","P2",null,null,1]
["LED白灯",null,null,null,"贴片LED","LED 0603W","LED3, LED4",null,null,2]
["LED-RGB",null,null,null,"贴片LED","LED-0606-GY","LED1, LED2",null,null,2]
["TM52F8276",null,null,null,"MCU","SOP20","U1",null,null,1]
["贴片触摸按键",null,null,null,"触摸按键","TB_10-贴片","TK1, TK2, TK3, TK4 ",null,null,4]
["单排针",null,null,null,"单排针",null,null,null,"定位柱",3]
[]
["MERC-0241  主板-板厚1.2mm"]
["需求","规格","建议物料","备选物料","类别","封装","位号","NC","备注","数量"]
["100nF/50V","100nF",null,null,"贴片电容","C0603","C4, C5, C8, C14, C15, C18",null,null,6]
["1nF/25V","1nF",null,null,"贴片电容","C0603","C1, C7, C13, C16, C19, C20, C21",null,null,7]
["1uF/25V","1uF",null,null,"贴片电容","C0603","C2",null,null,1]
["2.2uF/25V","2.2uF",null,null,"贴片电容","C0603","C9, C10, C11",null,null,3]
["10uF/25V","10uF",null,null,"贴片电容","C0805","C3, C12",null,null,2]
["100nF/500V","100nF",null,null,"贴片电容","C1206","C6",null,null,1]
["10nF/500V","10nF",null,null,"贴片电容","C1206","CY1",null,null,1]
["100nF/500V","100nF",null,null,"贴片电容","C1812","CH1",null,null,1]
["100uF/25V","100uF",null,null,"电解电容","CAP 2.0*5*11","EC3",null,null,1]
["47uF/400V","47uF",null,null,"电解电容","CAP 5.0*12.5*20","EC1, EC2",null,null,2]
["680nF","680nF",null,null,"安规电容","CAp-X2-P_10-12*13*8","CX1",null,null,1]
["10R","10R",null,null,"贴片电阻","R0603",null,"R19, R20, R21",null,0]
["68R/1%","68R/1%",null,null,"贴片电阻","R0603","R11, R12, R22, R29, R33, R34",null,null,6]
["270R/1%","270R/1%",null,null,"贴片电阻","R0603","R13, R14, R15, R23, R24, R25",null,null,6]
["330R","330R",null,null,"贴片电阻","R0603","R10, R47",null,null,2]
["1K/1%","1K/1%",null,null,"贴片电阻","R0603","R2, R44, R45",null,null,3]
["10K/1%","10K",null,null,"贴片电阻","R0603","R1, R16, R17, R18, R26, R27, R28, R46",null,null,8]
["20K","20K",null,null,"贴片电阻","R0603","R41",null,null,1]
["10R","10R",null,null,"贴片电阻","R0805","R7",null,null,1]
["110R","110R",null,null,"贴片电阻","R1206","R8, R9",null,null,2]
["200K/1%","200K",null,null,"贴片电阻","R1206","R3",null,null,1]
["560K/1%","560K",null,null,"贴片电阻","R1206","R37, R42",null,null,2]
["680K/1%","680K",null,null,"贴片电阻","R1206","R4, R6",null,null,2]
["300mR","300mR",null,null,"贴片采样电阻","R0805","R5",null,null,1]
["150mR/1%/250mW","150mR/1%/250mW","建议使用200ppm以内低温漂采样电阻，不少于1/4W",null,"贴片采样电阻","R1206","R30, R31, R32",null,null,3]
["DB307S","DB307S",null,null,"整流桥","DBS","DB1",null,"可以替换DB207S",1]
["3.15A/250V贴片",null,null,null,"一次性保险丝","FUSE-SMD_L6.1-W2.5","FS1",null,null,1]
["47uH","SMD,6x6.5mm",null,null,"功率电感","L1040-SMD-L11.6-W10.1","LS1",null,null,1]
["1mH/300mA","1mH,±20%,300mA,4.5Ω ",null,null,"功率电感","L6045S","L2",null,null,1]
["37S01",null,null,null,"MCU","LCM32F037","U6",null,null,1]
["US1MW",null,null,null,"超快恢复二极管","SOD-323",null,"D1, D2, D3",null,0]
["M3052","可控硅控制光耦",null,null,"光耦","SOP4_M","U4, U9",null,null,2]
["FM3313",null,null,null,"电机控制IC","SOP8_M","U5, U7, U8",null,null,3]
["HD1520",null,null,null,"ACDC电源","SOP8_M","U2",null,null,1]
["3H4_B",null,null,null,"过零光耦","SOP-4-P1.27","U1",null,null,1]
["78L05",null,null,null,"线性稳压器","SOT89_M","U3",null,null,1]
["YH5N50","N沟道,500V",null,null,"场效应管","TO252","Q1, Q2, Q3, Q4, Q5, Q6",null,null,6]
["BT138-800E",null,null,null,"可控硅","TO220A","BT1",null,null,1]
["7D471",null,null,null,"压敏电阻","VR","RV1",null,null,1]
["3D-9",null,null,null,"热敏电阻","NCT_7p5","NTC1",null,null,1]
["2Pin贴片端子","间距1.25，贴片",null,null,"贴片端子","CON-SMD_2P-P1.25-HC","P2",null,"NTC",1]
["4Pin贴片排母","2x2P-P2.00",null,null,"贴片端子","CON-SMD_2x2P-P2.00-PM","P1",null,null,1]
[]
[]
["线材"]
["3P电机线"]
["电机接地线"]
["电源线-N"]
["电源线-L"]